|  |
| --- |
| Difference Between NAAC & NBA Accreditation - Haq Se EngineerPREC LONIJai Shriram Engineering College (@JSREC09) / Twitter**JAI SHRIRAM ENGINEERING COLLEGE**  **TIRUPPUR – 638 660**  Approved by AICTE, New Delhi & Affiliated to Anna University, Chennai  Recognized by UGC & Accredited by NAAC and NBA (CSE and ECE) |

**DEPARTMENT OF**

**ELECTRONICS AND COMMUNICATION ENGINEERING**

**IBM - Naan Mudhalvan**

**Internet of Things**

**Group 3**

**Phase 1 - Project Submission**

**NAME : C.Ranganayaki**

**NM ID : au711221106027**

**YEAR : III**

**NOISE MONITORING SYSTEM**

**Introduction:**

A noise monitoring system is a technological solution designed to measure, analyze, and manage noise levels in various environments. These systems use sensors and equipment to capture sound data, which is then processed to assess noise pollution, compliance with regulations, or the impact of noise on people and the environment. Noise monitoring systems are widely used in urban planning, industrial settings, transportation, and public health to ensure sound quality and mitigate noise-related issues. They play a crucial role in maintaining environmental standards and improving the well-being of communities.



**Project definition:**

The Real-time Noise Monitoring System with Public Accessibility project aims to develop a comprehensive solution for monitoring and disseminating real-time noise level data in public areas through a user-friendly platform or mobile application. This project will leverage IoT (Internet of Things) sensors to continuously measure noise pollution in various urban and public spaces.

**Key Objectives**:

IOT Sensor Deployment: Install a network of IOT noise sensors strategically in public areas, including urban centers, parks, transportation hubs, and residential neighborhoods.

Data Collection:

Implement sensors capable of capturing noise levels at regular intervals. Ensure these sensors can measure noise across various frequencies to provide a holistic understanding of noise pollution.

Real-time Data Processing:

Develop a robust data processing and analytics system to collect, store, and process the noise data in real-time. This system should be able to identify trends, spikes, and unusual noise events.

User-Friendly Interface:

Create a user-friendly web platform or mobile application that displays real-time noise data in an easily understandable format. The interface should provide users with access to noise levels at specific locations and the ability to explore historical data.

Public Accessibility:

Make the noise level data accessible to the general public, local authorities, researchers, and urban planners. Ensure that the information is presented in a transparent and comprehensible manner.

Alerting Mechanism:

Implement an alerting system that can notify users and relevant authorities when noise levels exceed permissible limits, helping to address noise-related issues promptly.

Data Visualization:

Incorporate data visualization tools to present noise data through graphs, heatmaps, and other visual aids to help users grasp trends and patterns.

Data Security and Privacy:

Ensure the security and privacy of collected data, adhering to data protection regulations and best practices.

Community Engagement:

Encourage public engagement by soliciting feedback from users and involving the community in noise pollution mitigation efforts.

Data Processing Unit:

Design the system to be scalable, allowing for the addition of more sensors and features as needed to cover a wider geographic area.

Scability:

By successfully implementing this Real-time Noise Monitoring System with Public Accessibility project, it gives the expected result .

**Design thinking:**

**Project objectives:**

Real-time Noise Pollution Monitoring:

Deploy IOT sensors to continuously monitor noise levels in public areas. Collect and process noise data in real-time to provide up-to-the-minute insights into noise pollution levels

Public Awareness:

Create a user-friendly platform or mobile app to make noise data accessible to the public. Empower individuals and communities with real-time noise information to raise awareness about their local noise environment.

Noise Regulation Compliance:

Assist local authorities and organizations in monitoring and enforcing noise regulations Implement an alerting mechanism to notify authorities and the public when noise levels exceed permissible limits.

Improved Quality of Life:

Contribute to a quieter and more peaceful environment by addressing noise pollution. Enable urban planners and policymakers to make informed decisions to improve the quality of life for residents.

**Sensor design:**

Noise Sensors:

Develop compact and weather-resistant noise sensors capable of measuring noise levels across various frequencies accurately. Include the following features,

* Microphone for sound capture.
* Real-time data transmission capabilities.
* Power-efficient design for extended sensor life.
* Data encryption to ensure security.

Connectivity:

Use low-power, long-range communication protocols (e.g., LORA, NB-IOT) for seamless data transmission to a central server.

Power Source:

Implement a combination of battery and solar power to ensure continuous operation without the need for frequent maintenance.

Data Processing Unit:

Include a built-in processor to preprocess data locally before transmitting it to the central server, reducing the load on the network.

**Deployment Plan:**

Site Selection:

Identify key public areas where noise monitoring is crucial, including:

* Urban centers.
* Parks and recreational areas.
* Residential neighborhoods.
* Transportation hubs (airports, train stations, etc.).

Sensor Placement:

Install noise sensors at strategic locations within these areas, ensuring comprehensive coverage.

Sensors should be mounted at a height to avoid obstructions and vandalism.

Network Infrastructure:

* Set up a network infrastructure to support sensor communication.
* Install gateway devices to collect data from sensors and relay it to the central server.

Central Data Hub:

* Establish a central server for data aggregation and processing.
* Implement real-time data analysis to identify noise trends and anomalies.

User Interface:

* Create a user-friendly web platform or mobile app for data visualization and access.
* Ensure that the interface allows users to select specific locations and view real-time noise data.

Alerting System:

Develop an alerting mechanism to notify relevant authorities and the public when noise levels exceed prescribed limits.

Data Storage and Security:

* Store historical data securely for analysis and regulatory compliance.
* Implement robust data security measures to protect sensitive information.

Community Engagement:

* Involve local communities in the deployment process to raise awareness and gain support.
* Encourage feedback and participation to create a sense of ownership

**Noise pollution information platform:**

Real-time Noise Data:

* Access live noise level data from monitoring stations across the city.
* Visualize noise levels on a map, making it easy to identify noisy areas.

Personalized Alerts:

* Set noise level thresholds for specific locations and receive alerts when they are exceeded.
* Stay informed about noise events that matter to you.

Historical Data:

* View historical noise data to track trends and monitor improvements over time.
* Utilize data for research and advocacy efforts.

Community Engagement:

* Report noise disturbances directly through the app, enhancing community involvement.
* Connect with neighbors and local authorities to address noise concerns.

Educational Resources:

* Access noise pollution information, tips for reducing noise, and its impact on health.
* Raise awareness and promote responsible noise behavior.

User-Friendly Design:

* Intuitive interface for both web and mobile platforms.
* User profiles for personalized settings and data tracking.

Data Transparency:

Ensure transparency by providing information about monitoring locations, methodology, and data sources

**Integration approach:**

IOT Sensor Deployment:

* Install noise monitoring IOT sensors strategically throughout the target area.
* These sensors should be capable of capturing noise levels and other relevant environmental data.

Data Transmission Protocol:

* Utilize a standardized data transmission protocol such as MQTT (Message Queuing Telemetry Transport) for sensor-to-platform communication.
* MQTT is lightweight, efficient, and ideal for real-time data transfer.

Data Encryption:

* Implement data encryption mechanisms to ensure the security and integrity of transmitted data.
* Use industry-standard encryption protocols like HTTPS to protect data in transit.

Sensor Connectivity:

* Sensors should be equipped with multiple connectivity options, including Wi-Fi, cellular, or LPWAN (Low-Power Wide-Area Network) technologies.
* This ensures that sensors can transmit data reliably even in diverse environments.

Cloud-Based Data Storage:

* Store incoming sensor data in a scalable and secure cloud database.
* Employ cloud services like AWS, Azure, or Google Cloud to manage data storage and retrieval.

Data Processing:

* Implement real-time data processing pipelines to analyze incoming data for noise levels.
* Apply algorithms to filter and aggregate data, ensuring accuracy and reliability.

API Integration:

* Develop RESTful APIs to enable seamless communication between the sensor data storage and the Noise Pollution Information Platform.
* APIs facilitate data retrieval and visualization.

User Authentication and Authorization:

* Implement user authentication and authorization mechanisms to secure platform access.
* Users should have access to data relevant to their locations or areas of interest.

Real-Time Data Display:

* Integrate the processed sensor data into the platform’s user interface.
* Visualize noise levels on maps and provide customizable alerts to users.

Data Validation:

* Implement data validation checks to identify and handle outliers or erroneous sensor readings.
* Ensure data accuracy and reliability.

Scalability and Redundancy:

* Design the platform to be scalable to accommodate additional sensors and users.
* Implement redundancy to ensure platform availability and data integrity.

**Conclusion**:

This integration approach ensures the seamless connection of IOT sensors with the Noise Pollution Information Platform. By following this strategy, we can provide users with real-time, accurate noise pollution data, empowering them to make informed decisions and take actions to address noise-related issues effectively. This approach also lays the foundation for future expansion and enhancements to the platforms